Current Help System: PC-DMIS Settings Editor (View Core Help)

### Minimum Line Segment Length In MM

This value is used to control the minimum length for a line segment that is created from the segmentation process of a continuous scan. PC-DMIS uses internal functions to create line and arc segments that make up a continuous scan. Line segments that are shorter than this value will be eliminated from the scan data. This settings as well as the "MaximumArcSegmentRadiusInMM" and "MinimumArcSegmentRadiusInMM" settings help deal with noise in the scan line and provide more consistent segmentation.

Entry Name: MinimumLineSegmentLengthInMM

Entry Type: Real Number specifying maximum radius. Default value is 2.

User permission is required to change entry