Current Help System: PC-DMIS Settings Editor (View Core Help)

### Patch Boundary Crossings

Determines how many times a Patch scan can cross the selected boundary type before stopping the scan. For example, if you specify that the number of crossings is two, the scan will stop once the probe's BallCenter crosses the given condition’s surface (planar, spherical, cylindrical, conical etc.) two times.

Entry Name: PatchBoundaryCrossings

Entry Type: Whole Number specifying number of times. Default value is 1.

User permission is required to change entry