Current Help System: PC-DMIS Settings Editor (View Core Help)

### DCC XYZ2_2

Provides the default "Z" or "H" (height) value for the for the end point of a line auto feature. The value will represent Z value when the "Cartesian" value is set to TRUE (1), and H when it is set to FALSE (0). This value and the "DccXYZ2_0" and "DccXYZ2_1" values are used for Contact probes while the "Point2(XYZ)" values are used for Vision probes.

Entry Name: DccXYZ2_2

Entry Type: Real Number to specify the Z or H value. Default value is 0.

User permission is required to change entry