Current Help System: PC-DMIS Settings Editor (View Core Help)

### Probe Qual Vision Edge Strength

This value sets the minimum edge strength for a detected edge point to be used. This value is only used for Vision Probe Offset calibration. The data discrimination for edge strength occurs at a low level as each point is collected from the sensor, in this case the image processing. Points whose strength is too low are not passed up to the parent feature, such as a circle, for further processing, fitting, filtering, etc.

See the "Strength" value of the "Automatic Hit Target - Edge Parameter Set" topic in the "PC-DMIS Vision" help file.

Entry Name: ProbeQualVisionEdgeStrength

Entry Type: Whole Number to specify edge strength. Default value is 4.

User permission is required to change entry