Current Help System: PC-DMIS Settings Editor (View Core Help)

### Part Sensor Delay

This value will cause PC-DMIS to wait during part program execution before reading the Sensors to obtain the current temperatures. If zero is entered then there is no pause.

Entry Name: PartSensorDelay

Entry Type: Character String specifying seconds. Default value is 0.0.

User permission is required to change entry