Current Help System: PC-DMIS Settings Editor (View Core Help)

### DMIS Export Use Chorus Wrist Rotation

This option should be turned on if you are using a DEA CMM equipped with an IW42, CW43 or CW43L wrist. PC-DMIS follows Chorus conventions and adjusts the B rotation angle during the export of the SNSLCT statement. This option is automatically used when performing a ChorusDMIS export.

Entry Name: DMISExportUseChorusWristRotation

Entry Type: Whole Number to specify TRUE (1) or FALSE (0). Default value is 0.

User permission is required to change entry