Current Help System: PC-DMIS Settings Editor (View Core Help)

### Alternate Tessellation

This option will cause all CAD models imported from IGES, VDA, STEP, and DXF/DWG to be tessellated using the alternate tessellation algorithm. This option should be set to True for models that don't tessellate correctly with the default tessellation algorithm.

Entry Name: AlternateTessallation

Entry Type: True/False value. Default value is FALSE.

User permission is required to change entry