Current Help System: PC-DMIS Settings Editor (View Core Help)

### DCC Mode

Defines the Calibration method to be used during Dual Arm calibration. When this value is set to TRUE (1), PC-DMIS uses DCC mode that will allow you to supply the sphere positions and it will do all the motion under computer control. When this value is set to FALSE (0), PC-DMIS will prompt you to measure each sphere position using the CMM's jog box. Once you have taken the first hit on the top of the sphere, PC-DMIS will take the rest of hits in DCC mode.

Entry Name: DCCMode

Entry Type: Whole Number specifying DCC (1) or MANUAL (0). Default value is 0.

User permission is required to change entry