Current Help System: PC-DMIS Settings Editor (View Core Help)

### Probe Shank Check

This option should be set to TRUE (1), if you will be using a shank tip to take edge hits. With this option set to TRUE (1), PC-DMIS allows you to qualify the shank of the probe. You can also manipulate the other shank entries to determine how the shank is measured:

Important: Be aware that if you will be using a shank probe, you only need to do a shank calibration if you'll be taking edge hits.

Entry Name: ProbeShankCheck

Entry Type: Whole Number to specify TRUE (1) or FALSE (0). Default value is 0.

User permission is required to change entry

See Also: ProbeShankNumHits, ProbeShankOffset