Current Help System: PC-DMIS Settings Editor (View Core Help)

### External Rotab Protocol

This value sets the communications protocol for the serial connection to the rotary table controller. It specifies the comm port, baud rate, parity, data bits and stop bits settings.

Entry Name: ExternalRotabProtocol

Entry Type: Character String specifying communications protocol. Default value is “COM0 9600 N,8,1”.

User permission is required to change entry