Current Help System: PC-DMIS Settings Editor (View Core Help)

### Patch Dir Tech2 Axis

Specifies the axis to be used with Patch Scans where the PatchDirTech2 option is set to Body Axis (1). The available axes are X, Y, and Z. The cut plane that your probe will crisscross will be parallel to this axis.

Entry Name: PatchDirTech2Axis

Entry Type: Whole Number specifying axis number. Default value is 0.

User permission is required to change entry

Axis Key

0 | X
1 | Y
2 | Z