Current Help System: PC-DMIS Settings Editor (View Core Help)

### Probe Qual Vision ParCalibration Tolerance

As the ParFocal or ParCentral calibration measure the standard at each Magnification step, the results should be the same, or ‘close’, if the machine is well adjusted. If the measured results exceed this value, then the machine is considered grossly maladjusted.

Entry Name: ProbeQualVisionParCalibrationTolerance

Entry Type: Real Number to specify tolerance. Default value is 5.

User permission is required to change entry