Current Help System: PC-DMIS Settings Editor (View Core Help)

### Free X Move From Rack

Specifies the "X" value of the arm when it is placed in a "passing lane" in front of the rack. A "passing lane" defines a zone where the arm is free to move. To determine this value, use the jog box to move the arm to the passing lane in front of the rack.

Entry Name: FreeXMoveFromRack

Entry Type: Real Number to specify X value. Default value is 100.

User permission is required to change entry