Current Help System: PC-DMIS Settings Editor (View Core Help)

### DCC Diam

Defines the default Diameter value that will be used for circular auto features (circles, cones, cylinders and spheres). For a cone, this value represents the nominal diameter at the end of the cone where you've defined the X,Y, and Z location. This value is used for Contact probes while the "Diameter" value is used for Laser and Vision probes.

Entry Name: DccDiam

Entry Type: Real Number to specify diameter. Default value is 0.

User permission is required to change entry