Current Help System: PC-DMIS Settings Editor (View Core Help)

### External Probehead Init Timeout

Specifies a timeout for response to the initial attempt to communicate with the probe head when PC-DMIS is started. A value of 0.0 disables this timeout. If the timeout occurs, an error message will be display to indicate that the device is not responding.

Entry Name: ExternalProbeheadInitTimeout

Entry Type: Real Number specifying seconds. Default value is 2.

User permission is required to change entry