Current Help System: PC-DMIS Settings Editor (View Core Help)

### Cone Angle For Move Over Path

This value is the half angle of a cone around the probe tip that is used to determine how to move to avoid a collision. If the path direction at the point of a collision is within this cone of the tip vector, then a clearance move along the mount vector (arm vector) is attempted to avoid the collision. Otherwise a clearance move along the tip vector is attempted.

Entry Name: ConeAngleForMoveOverPath

Entry Type: Real Number to specify angle in degrees. Default value is 35.

User permission is required to change entry