Current Help System: PC-DMIS Settings Editor (View Core Help)

### DCC Spacer

Allows you to define the default value for the Spacer option that will be used when an Auto Feature is created. The Spacer value defines the distance from the nominal point location that PC-DMIS will use to measure a plane if sample hits are specified.

Entry Name: DccSpacer

Entry Type: Real Number to specify distance. Default value is 0.

User permission is required to change entry

If no value is entered, PC-DMIS uses a default distance.