Current Help System: PC-DMIS Settings Editor (View Core Help)

### Temp Sensor Numbers (0-3)

The Sensor Numbers values contain a list of one or more sensor numbers to be used for the given axis or part. These values are very important when reading temperatures from the controller because they must correspond to how the sensors are actually configured.

- Each sensor is a number in the range of 1 to 32.

- Items in the list can be either a single number or a range from first to last.

- Items are separated by either commas or left blank.

- The input allows up to 32 values for any axis or the part.

Entry Name: TempSensorNumbers(0-3)

Entry Type: Character String specifying sensor number. Default value is None ( ).

User permission is required to change entry

Number Key:

0 | X Axis
1 | Y Axis
2 | Z Axis
3 | Part

Note: For "manual" mode these numbers are relatively meaningless but at least one sensor number must be assigned for each axis and the part.