Current Help System: PC-DMIS Settings Editor (View Core Help)

### Sensor Tol Right

Determines the number of permissible missing pixels to the right of the current pixel and is still considered a continuous line. The Long Line value uses this value for measuring spheres and some cylinders..

Entry Name: SensorTolRight

Entry Type: Real Number to specify number of pixels. Default value is 0

User permission is required to change entry