Current Help System: PC-DMIS Settings Editor (View Core Help)

### Probe Qual Vision XY Illum

Stores the default XY Illumination value that is used in the Measure Vision Probe dialog box. This illumination source will be used for the XY measurements. Normally, the bottom or substage illumination for ring gage hole edge is used.

Entry Name: ProbeQualVisionXYIllum

Entry Type: Real Number specifying illumination source value. The default is -1.

User permission is required to change entry