Current Help System: PC-DMIS Settings Editor (View Core Help)

### DCC Measure Order

This value is used to determine the order that sample hits are taken for an edge point.

Entry Name: DccMeasureOrder

Entry Type: Whole Number to specify measure order. Default value is 0.

User permission is required to change this entry

Value Key:

0 | Surface | Surface measures the three hits, first on the surface, then on the edge.
1 | Edge | Edge measures the two hits, first on the edge then the surface.
2 | Both | Both measures the surface, then the edge, and then the surface again.