Current Help System: PC-DMIS Settings Editor (View Core Help)

### Sensor Points Density Type

Specifies the Density Type that is used for filter points laser scan.

Entry Name: SensorPointsDensityType

Entry Type: Whole Number specifying the Filter Density Type. Default value is 0.

User permission is required to change entry

Value Key:

0 | None
1 | Column Sampling Rate (CSR)
2 | Intelligent Density Management (IDM)