Current Help System: PC-DMIS Settings Editor (View Core Help)

### Probe Number of Data

Allows you to enter the number of readings taken when the machine is moving away from the object being measured. Defines the minimum number of data to be collected within the probing window defined by the ProbeUpperForce and ProbeLowerForce values.

Entry Name: ProbeNumberOfData

Entry Type: Character String specifying a number. Default value is 7.

User permission is required to change entry