Current Help System: PC-DMIS Settings Editor (View Core Help)

### Alternate Tip Mirror

When this value is set to FALSE, the IW42 (right-hand) mirrors like a PH-10. This option, when set to TRUE, is used to accommodate the use of a left-hand version of the IW42. Otherwise, one axis will be mirrored backwards.

Entry Name: AlternateTipMirror

Entry Type: True/False value. Default value is FALSE.

User permission is required to change entry