Current Help System: PC-DMIS Settings Editor (View Core Help)

### Avoid Table

Table Avoidance is active when this value is set to TRUE (1). This allows PC-DMIS to ascertain if the probe will come in contact with the table (or set plane) while in DCC mode.

Entry Name: AvoidTable

Entry Type: Whole Number to specify TRUE (1) or FALSE (0). Default value is 0.

User permission is required to change entry