Current Help System: PC-DMIS Settings Editor (View Core Help)

### Scan Dialog Indent 2

Allows you to set the indent on the top surface from the edge where the sample hits will be taken. This option is only available if ANGLE is selected from the "ScanDialogHitType" option.

Entry Name: ScanDialogIndent2

Entry Type: Real Number specifying distance. Default value is 0.1.

User permission is required to change entry