Current Help System: PC-DMIS Vision (View Core Help)

## Calibrating Vision Probes

Calibration for your Vision probe is accomplished from the Probe Utilities dialog box. In most cases, each of the calibrations should be completed before you can begin measuring with your Vision probe. To access this dialog box, select a probe that has already been added from the Edit Window and click F9 or select the Insert | Hardware Definition | Probe menu item.

Probe Utilities dialog box - Vision Probe specified

Define the Vision probe with the needed components then click Measure to access the Calibrate Vision Probe dialog box

Calibrate Vision Probe dialog box

The Calibrate Vision Probe dialog box allows you select and perform the following calibrations, which should be calibrated in the order listed below:

- Calibrate Optical Center

- Calibrate Optics

- Calibrate Illumination

- Calibrate Probe Offset

More:

A Note on Probe Definitions

Considerations for Vision Probes