Current Help System: PC-DMIS Vision (View Core Help)

#### Step 1: Define the Touch Trigger Probe and Two Tip Positions

The first thing you will need to do is define the correct probe, extensions, tip and tip positions for your touch trigger probe.

1. From the Probe Utilities dialog box (
   Insert | Hardware Definition | Probe), define the probe, extension, and tips in the Probe Description box.

2. Click the Add Angles button. The Add New Angles dialog box appears.

3. Add the A0B0C0 and A90B180C0 angles into the New Angles List.

4. Click OK to accept the tip angles specified in the Add New Angles dialog box. The angles now appear in the Active Tip List of the Probe Utilities dialog box.

Next Step...