Current Help System: PC-DMIS Vision (View Core Help)

#### Vector Point Field Definitions with NC-100

This is already covered in the "Vector Point Field Definitions" topic in the "Creating Auto Features" section. The following definition is specific to NC-100 video probes:

ACTL_THICKNESS = This value indicates the keyed in offset thickness of the measured data. Positive or negative values can be used.