NAME=CCD
Charge Coupled Device - This is one of the two main types of image sensors used in digital cameras.
NAME=CMMI
Standard CMM Interface such as a LEITZ.DLL
NAME=Fiducials
A point of reference. For example, In the case of a CAD file of a circuit board, these fiducials reference the location of soldering. These references may not exist in the CAD file.
NAME=Field of View
The FOV represents the view through the video camera. In the Live View, the FOV is everthing you see. In the CAD View, PC-DMIS Vision represents the FOV by a green rectangle that appears on top of the graphical image.
NAME=FOV
Field of View
NAME=HSI
Hardware Specific Interface
NAME=Image Tear
This is where "breaks" in the image occur due to the refresh rate not keeping up with the speed of movement.
NAME=Intensity Circle
The circle that is located in the middle of the Top light, Bottom light or segment of a ring light that shows the current intensity value for that light.
NAME=MSI
Multi Sensor Interface
NAME=NA
Numerical Aperture (NA) is a measure the light-gathering ability of a Vision device. NA is a measure of the number of highly diffracted image-forming light rays captured by the objective. Higher values of numerical aperture allow increasingly oblique rays to enter the objective front lens, producing a more highly resolved image.
NAME=Par-centricity
When the Focal XY Center of the optics is aligned with the Video Frame center through the zoom range.
NAME=Par-focality
When the focal clairity is consistant through the zoom range.
NAME=ROI
Region of Interest -  Targets are divided into multiple regions based upon the Field of View. Point detection will be determined for each ROI
NAME=Target
Individual regions that are used for point detection for the specified feature.
NAME=Tracker
The visual user interface to features that control the size of the circle, start angle, end angle, and orientation.
