Current Help System: PC-DMIS Vision (View Core Help)

#### Square Slot/Gap and Flush Type Definition

SQUARE SLOT = This type of feature allows the measurement of a square slot

GAP NORMAL = This type of feature allows the measurement of the gap and flush of a gap at the surface level of the fixed side.
The following description shows a generic case of point acquisition:
Gap Normal Point acquired by vision system

GAP DELTAZ = This request allows the measurement of a gap at a specified depth in respect to the fixed side of the part.
Gap &Flush measurement at a specified depth