Current Help System: PC-DMIS Vision (View Core Help)

#### Indent boxes

See also"Indent boxes" in the "Creating Auto Features" chaptersection.

Characteristic Point | PC-DMIS allows you to use two indent values, Indent 1 and Indent 2, for setting the offset distances of the Characteristic Point. PC-DMIS uses these offset distances to calculate a point location on each of the two surfaces of the angle in a Characteristic Point.

The indent boxes become available only after you select CHAR 1 from the Feat Type list.

Measure characteristic point using two theoretical distances

- The Indent 1 box allows you to set the offset distance from the point location to the sample hits on the first surface of the angle.

- The Indent 2 box allows you to set the offset distance from the point location for the sample hits on the second surface of the angle.