PC-Dmis 2010 MR1 Object Library | Send comments on this topic. | See Object Hierarchy Chart
TempComp Object Members
See Also Overview

Collapse All Expand All

# Public Methods

GetOrigin | Gets the reference origin
SetOrigin | Sets the reference origin

# Public Properties

HighThreshold | Read/Write: High temperature threshold Double value representing the high temperature threshold.
LowTheshold | Read/Write: Low temperature threshold Double value representing the low temperature threshold.
MaterialCoefficient | Read/Write: Material Coefficient Double value indicating the material coefficient.
RefTemp | Read/Write: Reference temperature Double value representing the reference temperature.
Sensors | Read/Write: Comma/Dash delimited list of sensor numbers (ie. '1-3,5') String value representing the list of sensors--by number--to be used for temperature compensation. The format of the list is a series of consecutive sensor numbers. The series are specified using the hyphen between the first number and the last number of the series. Each non-consecutive sensor or group of sensors is separated by the comma (or the typical separator for the given locale).

# See Also

TempComp Overview

© Wilcox Associates, Inc. All Rights Reserved.

© 2010 All Rights Reserved.