## Generic Feature Command Format

All generic features have XYZ and IJK values, and may have ANGLE, DIAMETER /RADIUS or DISTANCE values depending on the type assigned to the feature.

The Nominal / Measured Values toggle button indicates the values that will be used in the generic feature.

Command line in the Edit window (a cone is shown):

feature_name=GENERIC/TOG1,TOG2, TOG3, TOG4
NOM/XYZ,x_cord,y_cord,z_cord
MEAS/XYZ,x_cord,y_cord,z_cord
NOM/IJK,i_cord,j_cord,k_cord
MEAS/IJK,i_cord,j_cord,k_cord
[RADIUS/radius] | [DIAMETER/diameter]
[ANGLE/ang]
[DISTANCE/dist]

TOG1 = POINT, PLANE, LINE, CIRCLE, SPHERE, CYLINDER, CONE, SLOT or NONE

TOG2 = indicates whether the generic feature is alignment dependent, or independent.

TOG3 = indicates whether the feature uses Polar or Rectangular coordinates

TOG4 = indicates whether the feature is an IN (hole) or OUT (stud) feature.

[ ] = options shown in brackets are discretionary and are available based on the type assigned to the feature by TOG1. RADIUS and DIAMETER are mutually exclusive representations for the value represented as the radius or the diameter.