## Error Codes: Introduction

Error codes are used to alert the operator of warnings and error conditions that occur within the Coordinate Measuring System (CMS). The CMS consists of a coordinate measurement machine (CMM ), the CMM electronics, and a personal computer (PC) running MeasureMax+ or MaxLite.

The error codes in this section are specific to the Sheffield components which includes the CMM electronics and Measurement Library (MLB) commands.

Error codes are denoted by a group name, a hyphen and a number. A few examples are MP-523, MLB-010, and TempComp-200.

The error groups are:

- MLB

- MP

- DCC

- RCU

- TempComp