### MP-340 Offset angle error

The MP cannot process an establish offset command. Less than 2 points may be recorded, or the points may be recorded less than 2 mm apart.

This error only occurs when the MP front panel on an MP-30/35 system is used.

What you should do

1. To clear the error, press the MP CLEAR key on the MP front panel.

2. Record more points at least 2 mm apart.

3. Enter the offset command again.