### Default (I,J,K, Z) RMEAS Mode

When an Auto Feature has a relative measure feature associated with it (see "Relative Measurement area"), PC-DMIS measures the Auto Feature in a location that is adjusted to be on the plane of the RMEAS feature.

Example: Suppose you measured a plane (PLN), and an Auto Circle (CIR1) referenced the plane as its RMEAS feature. When you measure CIR1 PC-DMIS will measure it in the referenced plane (PLN). See "Math Process of the Default RMEAS Mode:".

The Edit window command for this option reads:

RMEAS/DEFAULT (I,J,K, Z)

This is the default and usual RMEAS mode for sheet metal features.

More:

Math Process of the Default (I,J,K, Z) RMEAS Mode: