### Decimal Placement Conventions

Please note the following information regarding decimal place conventions for constructed features:

- All vectors (i_vect, j_vect, k_vect) are represented by a maximum of 5 places to the right of the decimal.

- All lengths and distances (x_cord, y_cord, z_cord, diam, height, length, etc.) are represented by a maximum of 5 places to the right of the decimal.

- All angles are represented by a maximum of 5 places to the right of the decimal.

- If the decimal place is zero, then the number is represented as an integer.

Note: Decimal places can be changed through the Dimension tab (F5) on the Setup dialog box. Setting the decimal place limit inserts a DISPLAYPRECISION command in the Edit window. All features following this command conform to the number of decimal places specified.