#### Auto Set from Vector

Auto set from Vector area

This area remains unavailable for selection until you select the Stacked Rotary Tables option from the Rotary Table Setup dialog box. See "Defining the Rotary Table".

The Auto set from Vector area lets you select a feature from the Feature ID list. The active rotary table will automatically rotate to the best angle in order to make the probe normal to that feature.

Item | Description
Feature ID list | This contains all the features in the part program and allows you to choose the feature to which the table will rotate.
Target Vector IJK boxes | These boxes show the surface normal IJK for the selected feature. Alternately, you can type in your own IJK value. The rotary table will automatically rotate to be as close to normal as possible to the IJK contained in these boxes.