### BR - Turn Soft Probe On

The BR command enables the soft probe. The touch probe is disabled when this command is executed.

Command Format

MLString "BR"

Example

1. MLString "BR"

Input

None.

Results

The system enables the soft probe and starts including soft probe deflections as part of the tip position coordinate data.

Skip Action

Executes even when inside a skip block.

Error Messages

- MLB-080
  The soft probe has not been calibrated.