### LKDriver Interface

The LKDriver interface is used with the LK machines with LK3000 or LK2000 controllers. The common driver software must be obtained directly from LK. It must be installed and configured prior to attempting to install/use the PC-DMIS interface that utilizes it. The common driver DLL itself is named something similar to LKCMMDRV53.DLL, depending on the version number of the driver. There are also various other DLL’s that LK provides with the driver that must be present for the driver to work properly. The earliest version that can be used with the PC-DMIS interface is LKCMM21.DLL. Earlier versions are not compatible.

Before starting PC-DMIS, rename the lkdriver.dll to interfac.dll.

The Machine Option dialog box has three tabs for the LKDriver interface:

LK Driver tab

See the "LK Driver tab" topic.

Axis tab

See the "Assigning the Machine Axes" topic.

Debug tab

See the "Generating a Debug File" topic.

Note: Additional information for this interface is provided in the Machine Interface Installation Manual (MIIM).