#### Remove Outliers / Standard Deviation Multiple

For a Best Fit (BF) or Best Fit Recompensate (BFRE) plane you can choose to remove outliers based on the distance from the best fit feature. This allows the removal of anomalies that arise in the measurement process.

PC-DMIS first fits a plane to the data, then determines which points are outliers based on the standard deviation multiple. It then does the following:

1. Recalculates the best fit plane with those outliers removed.

2. Checks for outliers again.

3. Recalculates the best fit plane.

4. Continues repeating this process until no more outliers exist or until PC-DMIS cannot compute the plane (PC-DMIS can't compute the plane if there are fewer than 3 data points).