#### Additional Information on the Machine's Home Position area

These three boxes define the home position of the machine. The x, y, z values define where the home position is for the machine. The center of the machine base is 0,0,0. But these coordinates are not used to show the home position on most machines. The x,y,z values are offset from the 0,0,0 machine base position.

For example, if the machine's dimensions are 1000, 700, and 700 with the actual home position in the upper left corner in back, the machines offsets would be: -350, 500, 350 for the 1st, 2nd, and 3rd axes respectively.

Note: The Home Position area is only editable for user-defined machines; you cannot use it for machines supplied by PC-DMIS.