#### Auto Continue Execution if FindHole Fails

If you select the Auto Continue Execution if FindHole Fails check box, PC-DMIS allows you to automatically continue executing a part if the "FindHole" option found on the Auto Feature dialog box fails to find a hole.

In the past, when the “FindHole” option failed, PC-DMIS prompted you to place the probe in the center of the hole to continue running the part program. However, with the Auto Continue Execution if FindHole Fails check box selected, PC-DMIS automatically prints an error message to the report and continues running the remaining part program.

For more specific information on Find Hole, see the "Find Hole Check Box" topic in the "Creating Auto Features" section.