### Theodole Interface

The Theodole interface is used with a Theodolite machine.

Before starting PC-DMIS, rename the theodole.dll to interfac.dll.

The Machine Option dialog box has four tabs for the Theodole interface:

Controller tab

See the "Setting the Communication Protocol" topic. Default value is Comm Port 1, 19200 Baud, Even parity, 7 data bits, and 1 stop bit.

Axis tab

See the "Assigning the Machine Axes" topic.

Debug tab

See the "Generating a Debug File" topic.

Note: Additional information for this interface is provided in the Machine Interface Installation Manual (MIIM).