#### Use Automotive Deviation Letters

The Use Automotive Deviation Letters check box causes PC-DMIS to add a letter after the deviation number in Location and True Position dimension reports. PC-DMIS inserts the letter

· F when the feature deviates in the direction of the front of the car.

· B when the feature deviates in the direction of the back of the car.

· I when the feature deviates towards the centerline of the car (meaning the car is too narrow).

· O when the feature deviates away from the centerline of the car (meaning the car is too wide).

· H when the feature deviates towards the top of the car.

· L when the feature deviates towards the bottom of the car.

Map of Automotive Deviation Letters

These letters are added to the Location and True Position dimensions just following the deviation numbers reported. These deviation letters also appear inside the Report window for the appropriate dimensions.

Automotive Deviation Letters in Command Mode

Automotive Deviation Letters in Report Window