#### Step 2 Enter Corner Point Values

Type the X, Y, and Z values for Corner 1 and Corner 2. You can read in the probe's current into the selected corner point by clicking the Read Position button.

Defining two corners sets up the exclusion zone; be sure to select the corner points that will correctly define the exclusion zone. The two points (corner 1 and corner 2) represent two corners that are diagonal from each other.

A rectangular zone can be created in 3D space from two points if you use the current coordinate system to create the sides. A combination of different parts of the two points can construct the eight points needed to form the rectangular area.

Example:

First corner = X1, Y1, Z1
Second corner = X2, Y2, Z2
Third corner = X1, Y1, Z2
Forth corner = X1, Y2, Z1
Fifth corner = X1, Y2, Z2
Sixth corner = X2, Y1, Z1
Seventh corner = X2, Y1, Z2
Eight corner = X2, Y2, Z1