#### Equally Spaced Angles Data

The Add Angles button associated with these boxes automatically marks all of the requested equally spaced AB positions in the New Angles List box. The default position for the probe configuration is automatically included in the final list. A PH9 pointing straight down (A=0°, B=any°) is automatically defined and therefore doesn't need to be re-defined in this dialog box.

PC-DMIS easily allows you to measure all the AB positions from 0° to 90° in the A axis with 15° increments and from -180° to 180° in the B axis with 45° increments.

A axis angle range ¾ Front view of CMM with B = 90°.

B axis angle range¾top view with A = 90° | 1 - Front 2 - B Axis

To add angles to the New Angles List box:

1. Enter the necessary information in each available angle box (Starting A, Ending A, Increment in A, Starting B, Ending B, Increment in B).

2. Click the Add Angles button and PC-DMIS will automatically display the requested AB orientations, in the New Angles List box.

AB orientations displayed in the New Angles List box