Current Help System: PC-DMIS CMM (View Core Help)

###

### Working with Contact Auto Move Properties

Contact Auto Move Properties tab

This tab becomes visible when you have the Auto Feature dialog box open and a contact probe is enabled.

The Contact Auto Move Properties tab contains items that allow you to change Auto Move properties for Auto Features that use contact probes.

Auto Moves are special moves added to your feature's path lines to help PC-DMIS avoid driving the probe through your feature when it actually measures it.

This tab contains the following items:

Item | Description
Avoidance Move | This list lets you choose the type of Avoidance Move for your current Auto Feature. This list contains these items: NO - There will be no Avoidance Moves used for the current feature. BEFORE - Before PC-DMIS measures the first hit on the current feature, it will first move to the specified distance above the first hit. View Demo

AFTER - After PC-DMIS measures the last hit on the current feature, it will move to the specified distance above the last hit. View Demo

BOTH - Applies the Avoidance Move distance to the path lines both before and after PC-DMIS measures the feature.

Distance | This specifies the distance above the first probing or last probing to which the probe will move during execution.