Current Help System: PC-DMIS Fixturing (View Core Help)

#### Mount Points Tab

Mount Points - Dual Arm Setup

The values for both arms are the same. The Read Position command should only be done from the Master computer. Click Read Position for Arm 1 and Arm 2 to collect the values for the XYZ position. Click Read Position for Arm 1 Gripper and Arm 2 Gripper to collect the values for XYZ position.